**For the process capacity simulation performed in class;**

* Where is the bottleneck?
* What is the capacity of the process? Please explain.
* Does actual throughput time (stopwatch) equal expected throughput time (Little’s Law)? Why or why not?
* How could the exit rate be improved?
* How could throughput time be reduced?